From 2c02075a8ec5223bc4cbcc9561eb91e28d46a9e5 Mon Sep 17 00:00:00 2001
From: "Cui,Lili" <lili.cui@intel.com>
Date: Tue, 28 Sep 2021 11:13:33 +0800
Subject: [PATCH] x86: Print {bad} on invalid broadcast in OP_E_memory

Don't print broadcast for scalar_mode, and print {bad} for invalid broadcast.

gas/

	PR binutils/28381
	* testsuite/gas/i386/bad-bcast.s: Add a new testcase.
	* testsuite/gas/i386/bad-bcast.d: Likewise.
	* testsuite/gas/i386/bad-bcast-intel.d: New.

opcodes/

	PR binutils/28381
	* i386-dis.c (static struct): Add no_broadcast.
	(OP_E_memory): Mark invalid broadcast with no_broadcast=1 and Print "{bad}"for it.
	(intel_operand_size): mark invalid broadcast with no_broadcast=1.
	(OP_XMM): Mark scalar_mode with no_broadcast=1.

diff --git a/gas/testsuite/gas/i386/bad-bcast-intel.d b/gas/testsuite/gas/i386/bad-bcast-intel.d
new file mode 100644
index 00000000000..29de3de299c
--- /dev/null
+++ b/gas/testsuite/gas/i386/bad-bcast-intel.d
@@ -0,0 +1,15 @@
+#source: bad-bcast.s
+#objdump: -dw -Mintel
+#name: Disassemble bad broadcast (Intel mode)
+
+.*: +file format .*
+
+Disassembly of section .text:
+
+0+ <.text>:
+[ 	]*[a-f0-9]+:[ 	]*62 c3 8c 1d 66\s*\(bad\)
+[ 	]*[a-f0-9]+:[ 	]*90\s*nop
+[ 	]*[a-f0-9]+:[ 	]*66 90\s*xchg   ax,ax
+[ 	]*[a-f0-9]+:[ 	]*66 90\s*xchg   ax,ax
+[ 	]*[a-f0-9]+:[ 	]*62 c1 ff 38 2a 20\s*vcvtsi2sd xmm4,xmm0,\[eax\]{bad}
+#pass
diff --git a/gas/testsuite/gas/i386/bad-bcast.d b/gas/testsuite/gas/i386/bad-bcast.d
index 9fc474a42ff..4f829259994 100644
--- a/gas/testsuite/gas/i386/bad-bcast.d
+++ b/gas/testsuite/gas/i386/bad-bcast.d
@@ -7,8 +7,8 @@
 Disassembly of section .text:
 
 0+ <.text>:
- +[a-f0-9]+:	62                   	.byte 0x62
- +[a-f0-9]+:	c3                   	ret    
- +[a-f0-9]+:	8c 1d 66 90 66 90    	mov    %ds,0x90669066
- +[a-f0-9]+:	66 90                	xchg   %ax,%ax
-#pass
+ +[a-f0-9]+:	62 c3 8c 1d 66\s+\(bad\)
+ +[a-f0-9]+:	90\s+nop
+ +[a-f0-9]+:	66 90\s+xchg   %ax,%ax
+ +[a-f0-9]+:	66 90\s+xchg   %ax,%ax
+ +[a-f0-9]+:	62 c1 ff 38 2a 20\s+vcvtsi2sd \(%eax\){bad},%xmm0,%xmm4
diff --git a/gas/testsuite/gas/i386/bad-bcast.s b/gas/testsuite/gas/i386/bad-bcast.s
index 3e49b2238ed..6c55dcbbbd8 100644
--- a/gas/testsuite/gas/i386/bad-bcast.s
+++ b/gas/testsuite/gas/i386/bad-bcast.s
@@ -1,3 +1,5 @@
 	.text
 # Invalid 16-bit broadcast with EVEX.W == 1.
 	.byte 0x62, 0xc3, 0x8c, 0x1d, 0x66, 0x90, 0x66, 0x90, 0x66, 0x90
+# Invalid vcvtsi2sd with EVEX.b == 1.
+	.byte 0x62,0xc1,0xff,0x38,0x2a,0x20
diff --git a/gas/testsuite/gas/i386/i386.exp b/gas/testsuite/gas/i386/i386.exp
index 80959726d0e..680259b1c4e 100644
--- a/gas/testsuite/gas/i386/i386.exp
+++ b/gas/testsuite/gas/i386/i386.exp
@@ -646,6 +646,7 @@ if [gas_32_check] then {
 	run_dump_test "dw2-compress-2"
 	run_dump_test "dw2-compressed-2"
 
+	run_dump_test "bad-bcast-intel"
 	run_dump_test "bad-bcast"
 	run_dump_test "bad-size"
 
diff --git a/opcodes/i386-dis.c b/opcodes/i386-dis.c
index aa292233d4d..926f776de88 100644
--- a/opcodes/i386-dis.c
+++ b/opcodes/i386-dis.c
@@ -2422,6 +2422,7 @@ static struct
     int zeroing;
     int ll;
     int b;
+    int no_broadcast;
   }
 vex;
 static unsigned char need_vex;
@@ -11059,23 +11060,25 @@ intel_operand_size (int bytemode, int sizeflag)
 {
   if (vex.b)
     {
-      switch (bytemode)
-	{
-	case x_mode:
-	case evex_half_bcst_xmmq_mode:
-	  if (vex.w)
-	    oappend ("QWORD PTR ");
-	  else
-	    oappend ("DWORD PTR ");
-	  break;
-	case xh_mode:
-	case evex_half_bcst_xmmqh_mode:
-	case evex_half_bcst_xmmqdh_mode:
-	  oappend ("WORD PTR ");
-	  break;
-	default:
-	  abort ();
-	}
+      if (!vex.no_broadcast)
+	switch (bytemode)
+	  {
+	  case x_mode:
+	  case evex_half_bcst_xmmq_mode:
+	    if (vex.w)
+	      oappend ("QWORD PTR ");
+	    else
+	      oappend ("DWORD PTR ");
+	    break;
+	  case xh_mode:
+	  case evex_half_bcst_xmmqh_mode:
+	  case evex_half_bcst_xmmqdh_mode:
+	    oappend ("WORD PTR ");
+	    break;
+	  default:
+	    vex.no_broadcast = 1;
+	    break;
+	  }
       return;
     }
   switch (bytemode)
@@ -11908,69 +11911,71 @@ OP_E_memory (int bytemode, int sizeflag)
   if (vex.b)
     {
       evex_used |= EVEX_b_used;
-      if (bytemode == xh_mode)
-        {
-          if (vex.w)
-            {
-	      oappend ("{bad}");
-            }
-          else
-            {
-              switch (vex.length)
-                {
-                case 128:
-                  oappend ("{1to8}");
-                  break;
-                case 256:
-                  oappend ("{1to16}");
-                  break;
-                case 512:
-                  oappend ("{1to32}");
-                  break;
-                default:
-		  abort ();
-                }
-            }
-        }
-      else if (vex.w
-	  || bytemode == evex_half_bcst_xmmqdh_mode
-	  || bytemode == evex_half_bcst_xmmq_mode)
+      if (!vex.no_broadcast)
 	{
-	  switch (vex.length)
+	  if (bytemode == xh_mode)
 	    {
-	    case 128:
-	      oappend ("{1to2}");
-	      break;
-	    case 256:
-	      oappend ("{1to4}");
-	      break;
-	    case 512:
-	      oappend ("{1to8}");
-	      break;
-	    default:
-	      abort ();
+	      if (vex.w)
+		oappend ("{bad}");
+	      else
+		{
+		  switch (vex.length)
+		    {
+		    case 128:
+		      oappend ("{1to8}");
+		      break;
+		    case 256:
+		      oappend ("{1to16}");
+		      break;
+		    case 512:
+		      oappend ("{1to32}");
+		      break;
+		    default:
+		      abort ();
+		    }
+		}
 	    }
-	}
-      else if (bytemode == x_mode
-	  || bytemode == evex_half_bcst_xmmqh_mode)
-	{
-	  switch (vex.length)
+	  else if (vex.w
+		   || bytemode == evex_half_bcst_xmmqdh_mode
+		   || bytemode == evex_half_bcst_xmmq_mode)
 	    {
-	    case 128:
-	      oappend ("{1to4}");
-	      break;
-	    case 256:
-	      oappend ("{1to8}");
-	      break;
-	    case 512:
-	      oappend ("{1to16}");
-	      break;
-	    default:
-	      abort ();
+	      switch (vex.length)
+		{
+		case 128:
+		  oappend ("{1to2}");
+		  break;
+		case 256:
+		  oappend ("{1to4}");
+		  break;
+		case 512:
+		  oappend ("{1to8}");
+		  break;
+		default:
+		  abort ();
+		}
+	    }
+	  else if (bytemode == x_mode
+		   || bytemode == evex_half_bcst_xmmqh_mode)
+	    {
+	      switch (vex.length)
+		{
+		case 128:
+		  oappend ("{1to4}");
+		  break;
+		case 256:
+		  oappend ("{1to8}");
+		  break;
+		case 512:
+		  oappend ("{1to16}");
+		  break;
+		default:
+		  abort ();
+		}
 	    }
+	  else
+	    vex.no_broadcast = 1;
 	}
-      else
-	/* If operand doesn't allow broadcast, vex.b should be 0.  */
+      if (vex.no_broadcast)
 	oappend ("{bad}");
     }
 }
@@ -12685,6 +12690,8 @@ OP_XMM (int bytemode, int sizeflag ATTRIBUTE_UNUSED)
 
   if (bytemode == tmm_mode)
     modrm.reg = reg;
+  else if (bytemode == scalar_mode)
+    vex.no_broadcast = 1;
 
   print_vector_reg (reg, bytemode);
 }
-- 
2.33.0

