From 3907f30765bd5ca0d973c0b828de210b3d87713a Mon Sep 17 00:00:00 2001
From: Huisong Li <lihuisong@huawei.com>
Date: Fri, 21 Oct 2022 15:36:34 +0800
Subject: [PATCH 158/189] net/hns3: fix types in IPv6 SCTP fields

Fix spelling errors about IPV6-SCTP macro.

Fixes: 1bc633c34008 ("net/hns3: enable RSS for IPv6-SCTP dst/src port fields")
Cc: stable@dpdk.org

Signed-off-by: Huisong Li <lihuisong@huawei.com>
Signed-off-by: Dongdong Liu <liudongdong3@huawei.com>
---
 drivers/net/hns3/hns3_rss.c | 12 ++++++------
 1 file changed, 6 insertions(+), 6 deletions(-)

diff --git a/drivers/net/hns3/hns3_rss.c b/drivers/net/hns3/hns3_rss.c
index e7e114727f..6d71ee94a9 100644
--- a/drivers/net/hns3/hns3_rss.c
+++ b/drivers/net/hns3/hns3_rss.c
@@ -57,8 +57,8 @@ enum hns3_tuple_field {
 	HNS3_RSS_FIELD_IPV6_UDP_EN_IP_S,
 
 	/* IPV6_SCTP ENABLE FIELD */
-	HNS3_RSS_FILED_IPV6_SCTP_EN_SCTP_D = 48,
-	HNS3_RSS_FILED_IPV6_SCTP_EN_SCTP_S,
+	HNS3_RSS_FIELD_IPV6_SCTP_EN_SCTP_D = 48,
+	HNS3_RSS_FIELD_IPV6_SCTP_EN_SCTP_S,
 	HNS3_RSS_FIELD_IPV6_SCTP_EN_IP_D,
 	HNS3_RSS_FIELD_IPV6_SCTP_EN_IP_S,
 	HNS3_RSS_FIELD_IPV6_SCTP_EN_SCTP_VER,
@@ -135,9 +135,9 @@ static const struct {
 	{ RTE_ETH_RSS_NONFRAG_IPV6_SCTP | RTE_ETH_RSS_L3_DST_ONLY,
 	  BIT_ULL(HNS3_RSS_FIELD_IPV6_SCTP_EN_IP_D) },
 	{ RTE_ETH_RSS_NONFRAG_IPV6_SCTP | RTE_ETH_RSS_L4_SRC_ONLY,
-	  BIT_ULL(HNS3_RSS_FILED_IPV6_SCTP_EN_SCTP_S) },
+	  BIT_ULL(HNS3_RSS_FIELD_IPV6_SCTP_EN_SCTP_S) },
 	{ RTE_ETH_RSS_NONFRAG_IPV6_SCTP | RTE_ETH_RSS_L4_DST_ONLY,
-	  BIT_ULL(HNS3_RSS_FILED_IPV6_SCTP_EN_SCTP_D) },
+	  BIT_ULL(HNS3_RSS_FIELD_IPV6_SCTP_EN_SCTP_D) },
 	{ RTE_ETH_RSS_IPV6 | RTE_ETH_RSS_L3_SRC_ONLY,
 	  BIT_ULL(HNS3_RSS_FIELD_IPV6_NONFRAG_IP_S) },
 	{ RTE_ETH_RSS_IPV6 | RTE_ETH_RSS_L3_DST_ONLY,
@@ -185,8 +185,8 @@ static const struct {
 	  BIT_ULL(HNS3_RSS_FIELD_IPV6_UDP_EN_UDP_D) },
 	{ RTE_ETH_RSS_NONFRAG_IPV6_SCTP, BIT_ULL(HNS3_RSS_FIELD_IPV6_SCTP_EN_IP_S) |
 	  BIT_ULL(HNS3_RSS_FIELD_IPV6_SCTP_EN_IP_D) |
-	  BIT_ULL(HNS3_RSS_FILED_IPV6_SCTP_EN_SCTP_D) |
-	  BIT_ULL(HNS3_RSS_FILED_IPV6_SCTP_EN_SCTP_S) |
+	  BIT_ULL(HNS3_RSS_FIELD_IPV6_SCTP_EN_SCTP_D) |
+	  BIT_ULL(HNS3_RSS_FIELD_IPV6_SCTP_EN_SCTP_S) |
 	  BIT_ULL(HNS3_RSS_FIELD_IPV6_SCTP_EN_SCTP_VER) },
 	{ RTE_ETH_RSS_IPV6,
 	  BIT_ULL(HNS3_RSS_FIELD_IPV6_NONFRAG_IP_S) |
-- 
2.23.0

