From 1c230057a50db378f46e86e6f7fbcf8266e62fba Mon Sep 17 00:00:00 2001
From: Jie Hai <haijie1@huawei.com>
Date: Thu, 26 Sep 2024 20:42:45 +0800
Subject: [PATCH] net/hns3: fix dump counter of registers

[ upstream commit e9b82b4d54c019973ffcb5f404ba920494f70513 ]

Since the driver dumps the queue interrupt registers according
to the intr_tqps_num, the counter should be the same.

Fixes: acb3260fac5c ("net/hns3: fix dump register out of range")
Fixes: 936eda25e8da ("net/hns3: support dump register")
Cc: stable@dpdk.org

Signed-off-by: Jie Hai <haijie1@huawei.com>
Acked-by: Huisong Li <lihuisong@huawei.com>
Acked-by: Chengwen Feng <fengchengwen@huawei.com>
---
 drivers/net/hns3/hns3_regs.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/drivers/net/hns3/hns3_regs.c b/drivers/net/hns3/hns3_regs.c
index 53d829a..d9c5464 100644
--- a/drivers/net/hns3/hns3_regs.c
+++ b/drivers/net/hns3/hns3_regs.c
@@ -127,7 +127,7 @@ hns3_get_regs_length(struct hns3_hw *hw, uint32_t *length)
 	tqp_intr_lines = sizeof(tqp_intr_reg_addrs) / REG_LEN_PER_LINE + 1;
 
 	len = (cmdq_lines + common_lines + ring_lines * hw->tqps_num +
-	      tqp_intr_lines * hw->num_msi) * REG_NUM_PER_LINE;
+	      tqp_intr_lines * hw->intr_tqps_num) * REG_NUM_PER_LINE;
 
 	if (!hns->is_vf) {
 		ret = hns3_get_regs_num(hw, &regs_num_32_bit, &regs_num_64_bit);
-- 
2.33.0

