From 3111c03a6329f87d84f5938dc2d371a9f7820198 Mon Sep 17 00:00:00 2001
From: Dengdui Huang <huangdengdui@huawei.com>
Date: Wed, 3 Apr 2024 18:16:19 +0800
Subject: [PATCH 37/42] net/hns3: fix offload flag of IEEE 1588

[ upstream commit 5fde4c41f26d2ad607935b76b528e1b64727b5c7 ]

Currently, the RTE_MBUF_F_RX_IEEE1588_TMST offload flag will
not be set when the scatter algorithm is used.
This patch fixes it.

Fixes: 4801f0403b58 ("net/hns3: fix IEEE 1588 PTP for scalar scattered Rx")
Cc: stable@dpdk.org

Signed-off-by: Dengdui Huang <huangdengdui@huawei.com>
Signed-off-by: Jie Hai <haijie1@huawei.com>
---
 drivers/net/hns3/hns3_rxtx.c | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

diff --git a/drivers/net/hns3/hns3_rxtx.c b/drivers/net/hns3/hns3_rxtx.c
index 04ae8dc..dc5246b 100644
--- a/drivers/net/hns3/hns3_rxtx.c
+++ b/drivers/net/hns3/hns3_rxtx.c
@@ -2668,6 +2668,7 @@ hns3_recv_scattered_pkts(void *rx_queue,
 			continue;
 		}
 
+		first_seg->ol_flags = 0;
 		if (unlikely(bd_base_info & BIT(HNS3_RXD_TS_VLD_B)))
 			hns3_rx_ptp_timestamp_handle(rxq, first_seg, timestamp);
 
@@ -2697,7 +2698,7 @@ hns3_recv_scattered_pkts(void *rx_queue,
 
 		first_seg->port = rxq->port_id;
 		first_seg->hash.rss = rte_le_to_cpu_32(rxd.rx.rss_hash);
-		first_seg->ol_flags = RTE_MBUF_F_RX_RSS_HASH;
+		first_seg->ol_flags |= RTE_MBUF_F_RX_RSS_HASH;
 		if (unlikely(bd_base_info & BIT(HNS3_RXD_LUM_B))) {
 			first_seg->hash.fdir.hi =
 				rte_le_to_cpu_16(rxd.rx.fd_id);
-- 
2.33.0

