From 6963b0641d446209018f0fdc6cd773c92b3f4612 Mon Sep 17 00:00:00 2001
From: Chengwen Feng <fengchengwen@huawei.com>
Date: Sat, 12 Oct 2024 17:17:34 +0800
Subject: [PATCH] dmadev: fix potential null pointer access

[ upstream commit e5389d427ec43ab805d0a1caed89b63656fd7fde ]

When rte_dma_vchan_status(dev_id, vchan, NULL) is called, a null pointer
access is triggered.
This patch adds the null pointer checker.

Fixes: 5e0f85912754 ("dmadev: add channel status check for testing use")
Cc: stable@dpdk.org

Signed-off-by: Chengwen Feng <fengchengwen@huawei.com>
---
 lib/dmadev/rte_dmadev.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/lib/dmadev/rte_dmadev.c b/lib/dmadev/rte_dmadev.c
index 7729519..8a010c4 100644
--- a/lib/dmadev/rte_dmadev.c
+++ b/lib/dmadev/rte_dmadev.c
@@ -722,7 +722,7 @@ rte_dma_vchan_status(int16_t dev_id, uint16_t vchan, enum rte_dma_vchan_status *
 {
 	struct rte_dma_dev *dev = &rte_dma_devices[dev_id];
 
-	if (!rte_dma_is_valid(dev_id))
+	if (!rte_dma_is_valid(dev_id) || status == NULL)
 		return -EINVAL;
 
 	if (vchan >= dev->data->dev_conf.nb_vchans) {
-- 
2.33.0

