From d4bab55077c6a77bd80cb12a8b0d28020ef412a9 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Sebastian=20Dr=C3=B6ge?= <sebastian@centricular.com>
Date: Tue, 24 Sep 2024 09:50:34 +0300
Subject: [PATCH] qtdemux: Skip zero-sized boxes instead of stopping to look at
 further boxes

A zero-sized box is not really a problem and can be skipped to look at any
possibly following ones.

BMD ATEM devices specifically write a zero-sized bmdc box in the sample
description, followed by the avcC box in case of h264. Previously the avcC box
would simply not be read at all and the file would be unplayable.

Part-of: <https://gitlab.freedesktop.org/gstreamer/gstreamer/-/merge_requests/7564>
---
 .../gst-plugins-good/gst/isomp4/qtdemux.c     | 54 ++++++++++++-------
 1 file changed, 36 insertions(+), 18 deletions(-)

--- a/gst/isomp4/qtdemux.c
+++ b/gst/isomp4/qtdemux.c
@@ -11384,9 +11384,12 @@ qtdemux_parse_trak (GstQTDemux * qtdemux
               else
                 size = len - 0x8;
 
-              if (size < 1)
-                /* No real data, so break out */
-                break;
+              /* No real data, so skip */
+              if (size < 1) {
+                len -= 8;
+                avc_data += 8;
+                continue;
+              }
 
               switch (QT_FOURCC (avc_data + 0x4)) {
                 case FOURCC_avcC:
@@ -11501,9 +11504,12 @@ qtdemux_parse_trak (GstQTDemux * qtdemux
               else
                 size = len - 0x8;
 
-              if (size < 1)
-                /* No real data, so break out */
-                break;
+              /* No real data, so skip */
+              if (size < 1) {
+                len -= 8;
+                hevc_data += 8;
+                continue;
+              }
 
               switch (QT_FOURCC (hevc_data + 0x4)) {
                 case FOURCC_hvcC:
@@ -11925,9 +11931,12 @@ qtdemux_parse_trak (GstQTDemux * qtdemux
               else
                 size = len - 8;
 
-              if (size < 1)
-                /* No real data, so break out */
-                break;
+              /* No real data, so skip */
+              if (size < 1) {
+                len -= 8;
+                vc1_data += 8;
+                continue;
+              }
 
               switch (QT_FOURCC (vc1_data + 0x4)) {
                 case GST_MAKE_FOURCC ('d', 'v', 'c', '1'):
@@ -11967,9 +11976,12 @@ qtdemux_parse_trak (GstQTDemux * qtdemux
               else
                 size = len - 0x8;
 
-              if (size < 1)
-                /* No real data, so break out */
-                break;
+              /* No real data, so skip */
+              if (size < 1) {
+                len -= 8;
+                av1_data += 8;
+                continue;
+              }
 
               switch (QT_FOURCC (av1_data + 0x4)) {
                 case FOURCC_av1C:
@@ -12049,9 +12061,12 @@ qtdemux_parse_trak (GstQTDemux * qtdemux
               else
                 size = len - 0x8;
 
-              if (size < 1)
-                /* No real data, so break out */
-                break;
+              /* No real data, so skip */
+              if (size < 1) {
+                len -= 8;
+                vpcc_data += 8;
+                continue;
+              }
 
               switch (QT_FOURCC (vpcc_data + 0x4)) {
                 case FOURCC_vpcC:
@@ -12541,9 +12556,12 @@ qtdemux_parse_trak (GstQTDemux * qtdemux
             else
               size = len - 8;
 
-            if (size < 1)
-              /* No real data, so break out */
-              break;
+            /* No real data, so skip */
+            if (size < 1) {
+              len -= 8;
+              wfex_data += 8;
+              continue;
+            }
 
             switch (QT_FOURCC (wfex_data + 4)) {
               case GST_MAKE_FOURCC ('w', 'f', 'e', 'x'):
