From 6620c7cc62f11f1eda32c4b1c8006c0fdafb1c59 Mon Sep 17 00:00:00 2001
From: jipengfei <jipengfei_yewu@cmss.chinamobile.com>
Date: Thu, 24 Nov 2022 17:19:05 +0800
Subject: [PATCH 18/23] vmx: Require networkName for bridged and custom NICs
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

cherry-pick from db0564b4d34fb94fe59f04a4e411374ec1b6fc19

Commit 70768cda9740 marked this particular config string optional, but
forgot that two of the interface types still require this name to
exist.  Mark it as optional only if there is no connectionType.

Signed-off-by: Martin Kletzander <mkletzan@redhat.com>
Signed-off-by: jipengfei <jipengfei_yewu@cmss.chinamobile.com>
Reviewed-by: Reviewed-by: Ján Tomko <jtomko@redhat.com>
---
 src/vmx/vmx.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/src/vmx/vmx.c b/src/vmx/vmx.c
index fbc8366f2b..5f2ada6630 100644
--- a/src/vmx/vmx.c
+++ b/src/vmx/vmx.c
@@ -2667,7 +2667,7 @@ virVMXParseEthernet(virConfPtr conf, int controller, virDomainNetDefPtr *def)
         STRCASEEQ(connectionType, "bridged") ||
         STRCASEEQ(connectionType, "custom")) {
         if (virVMXGetConfigString(conf, networkName_name, &networkName,
-                                  true) < 0)
+                                  connectionType == NULL) < 0)
             goto cleanup;
 
         if (!networkName)
-- 
2.27.0

