From 4aec2da60ce3f639e31d81406c09d5c88b3b8f53 Mon Sep 17 00:00:00 2001
From: Florian Hahn <flo@fhahn.com>
Date: Wed, 20 Dec 2023 16:56:15 +0100
Subject: [PATCH 2/3] [ARM] Check all terms in emitPopInst when clearing
 Restored for LR. (#75527)

emitPopInst checks a single function exit MBB. If other paths also exit
the function and any of there terminators uses LR implicitly, it is not
save to clear the Restored bit.

Check all terminators for the function before clearing Restored.

This fixes a mis-compile in outlined-fn-may-clobber-lr-in-caller.ll
where the machine-outliner previously introduced BLs that clobbered LR
which in turn is used by the tail call return.

Alternative to #73553
---
 llvm/lib/Target/ARM/ARMFrameLowering.cpp | 30 +++++++++++++++++++++---
 llvm/lib/Target/ARM/ARMFrameLowering.h   |  3 +++
 2 files changed, 30 insertions(+), 3 deletions(-)

diff --git a/llvm/lib/Target/ARM/ARMFrameLowering.cpp b/llvm/lib/Target/ARM/ARMFrameLowering.cpp
index 4496d4928ebe..650f4650eef0 100644
--- a/llvm/lib/Target/ARM/ARMFrameLowering.cpp
+++ b/llvm/lib/Target/ARM/ARMFrameLowering.cpp
@@ -1645,9 +1645,6 @@ void ARMFrameLowering::emitPopInst(MachineBasicBlock &MBB,
         // Fold the return instruction into the LDM.
         DeleteRet = true;
         LdmOpc = AFI->isThumbFunction() ? ARM::t2LDMIA_RET : ARM::LDMIA_RET;
-        // We 'restore' LR into PC so it is not live out of the return block:
-        // Clear Restored bit.
-        Info.setRestored(false);
       }
 
       // If NoGap is true, pop consecutive registers and then leave the rest
@@ -2769,6 +2766,33 @@ void ARMFrameLowering::determineCalleeSaves(MachineFunction &MF,
   AFI->setLRIsSpilled(SavedRegs.test(ARM::LR));
 }
 
+void ARMFrameLowering::processFunctionBeforeFrameFinalized(
+    MachineFunction &MF, RegScavenger *RS) const {
+  TargetFrameLowering::processFunctionBeforeFrameFinalized(MF, RS);
+
+  MachineFrameInfo &MFI = MF.getFrameInfo();
+  if (!MFI.isCalleeSavedInfoValid())
+    return;
+
+  // Check if all terminators do not implicitly use LR. Then we can 'restore' LR
+  // into PC so it is not live out of the return block: Clear the Restored bit
+  // in that case.
+  for (CalleeSavedInfo &Info : MFI.getCalleeSavedInfo()) {
+    if (Info.getReg() != ARM::LR)
+      continue;
+    if (all_of(MF, [](const MachineBasicBlock &MBB) {
+          return all_of(MBB.terminators(), [](const MachineInstr &Term) {
+            return !Term.isReturn() || Term.getOpcode() == ARM::LDMIA_RET ||
+                   Term.getOpcode() == ARM::t2LDMIA_RET ||
+                   Term.getOpcode() == ARM::tPOP_RET;
+          });
+        })) {
+      Info.setRestored(false);
+      break;
+    }
+  }
+}
+
 void ARMFrameLowering::getCalleeSaves(const MachineFunction &MF,
                                       BitVector &SavedRegs) const {
   TargetFrameLowering::getCalleeSaves(MF, SavedRegs);
diff --git a/llvm/lib/Target/ARM/ARMFrameLowering.h b/llvm/lib/Target/ARM/ARMFrameLowering.h
index 16f2ce6bea6f..8d2b8beb9a58 100644
--- a/llvm/lib/Target/ARM/ARMFrameLowering.h
+++ b/llvm/lib/Target/ARM/ARMFrameLowering.h
@@ -59,6 +59,9 @@ public:
   void determineCalleeSaves(MachineFunction &MF, BitVector &SavedRegs,
                             RegScavenger *RS) const override;
 
+  void processFunctionBeforeFrameFinalized(
+      MachineFunction &MF, RegScavenger *RS = nullptr) const override;
+
   void adjustForSegmentedStacks(MachineFunction &MF,
                                 MachineBasicBlock &MBB) const override;
 
-- 
2.33.0

