From 5f8b5846741c965b1b5ad7a8ca2960b20565d192 Mon Sep 17 00:00:00 2001
From: suweifeng <suweifeng1@huawei.com>
Date: Thu, 10 Jun 2021 11:25:17 +0800
Subject: [PATCH 27/27] Change log level in poll timeout

Change to 'NOTICE' log level in poll timeout

Signed-off-by: suweifeng <suweifeng1@huawei.com>
---
 module/bdev/nvme/bdev_nvme_self.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/module/bdev/nvme/bdev_nvme_self.c b/module/bdev/nvme/bdev_nvme_self.c
index dc480ff..cba129e 100644
--- a/module/bdev/nvme/bdev_nvme_self.c
+++ b/module/bdev/nvme/bdev_nvme_self.c
@@ -36,7 +36,7 @@ void bdev_update_ch_timeout(struct nvme_bdev_poll_group *group)
 			poll_time = (poll_ticks * 1000ULL) / spdk_get_ticks_hz();
 			if (poll_time >= g_polltime_threshold) {
 				group->num_poll_timeout++;
-				SPDK_WARNLOG("group[%p] poll timeout in %ldms", group, poll_time);
+				SPDK_NOTICELOG("group[%p] poll timeout in %ldms", group, poll_time);
 			}
 		}
 		group->save_start_ticks = current_ticks;
-- 
2.33.0

