From ed9695ba9502b33f2f62b48beecfce1c4e70ad66 Mon Sep 17 00:00:00 2001
From: Jie Hai <haijie1@huawei.com>
Date: Thu, 26 Sep 2024 20:42:44 +0800
Subject: [PATCH] net/hns3: remove some basic address dump

[ upstream commit c8b7bec0ef23f53303c9cf03cfea44f1eb208738 ]

For security reasons, some address registers are not suitable
to be exposed, remove them.

Cc: stable@dpdk.org

Signed-off-by: Jie Hai <haijie1@huawei.com>
Acked-by: Huisong Li <lihuisong@huawei.com>
Acked-by: Chengwen Feng <fengchengwen@huawei.com>
---
 drivers/net/hns3/hns3_regs.c | 12 ++----------
 1 file changed, 2 insertions(+), 10 deletions(-)

diff --git a/drivers/net/hns3/hns3_regs.c b/drivers/net/hns3/hns3_regs.c
index be1be6a..53d829a 100644
--- a/drivers/net/hns3/hns3_regs.c
+++ b/drivers/net/hns3/hns3_regs.c
@@ -17,13 +17,9 @@
 
 static int hns3_get_dfx_reg_line(struct hns3_hw *hw, uint32_t *lines);
 
-static const uint32_t cmdq_reg_addrs[] = {HNS3_CMDQ_TX_ADDR_L_REG,
-					  HNS3_CMDQ_TX_ADDR_H_REG,
-					  HNS3_CMDQ_TX_DEPTH_REG,
+static const uint32_t cmdq_reg_addrs[] = {HNS3_CMDQ_TX_DEPTH_REG,
 					  HNS3_CMDQ_TX_TAIL_REG,
 					  HNS3_CMDQ_TX_HEAD_REG,
-					  HNS3_CMDQ_RX_ADDR_L_REG,
-					  HNS3_CMDQ_RX_ADDR_H_REG,
 					  HNS3_CMDQ_RX_DEPTH_REG,
 					  HNS3_CMDQ_RX_TAIL_REG,
 					  HNS3_CMDQ_RX_HEAD_REG,
@@ -44,9 +40,7 @@ static const uint32_t common_vf_reg_addrs[] = {HNS3_MISC_VECTOR_REG_BASE,
 					       HNS3_FUN_RST_ING,
 					       HNS3_GRO_EN_REG};
 
-static const uint32_t ring_reg_addrs[] = {HNS3_RING_RX_BASEADDR_L_REG,
-					  HNS3_RING_RX_BASEADDR_H_REG,
-					  HNS3_RING_RX_BD_NUM_REG,
+static const uint32_t ring_reg_addrs[] = {HNS3_RING_RX_BD_NUM_REG,
 					  HNS3_RING_RX_BD_LEN_REG,
 					  HNS3_RING_RX_EN_REG,
 					  HNS3_RING_RX_MERGE_EN_REG,
@@ -57,8 +51,6 @@ static const uint32_t ring_reg_addrs[] = {HNS3_RING_RX_BASEADDR_L_REG,
 					  HNS3_RING_RX_FBD_OFFSET_REG,
 					  HNS3_RING_RX_STASH_REG,
 					  HNS3_RING_RX_BD_ERR_REG,
-					  HNS3_RING_TX_BASEADDR_L_REG,
-					  HNS3_RING_TX_BASEADDR_H_REG,
 					  HNS3_RING_TX_BD_NUM_REG,
 					  HNS3_RING_TX_EN_REG,
 					  HNS3_RING_TX_PRIORITY_REG,
-- 
2.33.0

